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	Office of the Executive Engineer,
Nilphamari O& M Division,

BWDB, Nilphamari.

	
	
	


CORRIGENDUM TO THE NOTICE INVITING TENDERS

TENDER NOTICE NO. 02/2010-11

(Corrigendum Notice No.01)


This is for general information that the following Corrigendum has been made to the Notice Inviting Tender No. 02/2010-11 as circulated vide this office Memo. No. T-1/06(100) dated 02.01.2011.

	Description
	As per Tender floated
	As per this Corrigendum



	1
	2
	3

	"Item Sl. No. 2 of Section 6 containing the Tender Document of Tender Package No. N-25 & N-26"
	Supply and placing non-woven needle punched type geo textile filter of elongation>= 40%, horizontal and vertical permeability (under 2 kn/m2 pressure) = >3 × 10E-3 m/sec. and = > 5 × 10E-3 m/sec. respectively for effective erosion protection in hydraulic structures / river training works including local handling, placing in position, providing machine seamed joints (with 100% poly prop line or nylon thread) of 35 cm. lap in dry condition or minimum 100 cm lap under water including protecting the geo textile material  from UV ray and from any other damages including with supply of all materials , lobours, equipments etc. complete  as per direction of Engineer in charge.

( Geo textile delivered at site should be clearly labeled with brand name and grade printed at regular intervals accross the body of the fabric).                    

Mass = > 150gm/m2 , thickness ( Under 2 kpa pressure) = > 3.00 mm, EoS< = 0.08 mm, strip tensile strength = > 25 kn/m, grab strength = > 1650N, CBR puncture resistance = > 4000N.
	Supply and placing non-woven needle punched type geo textile fabric as filter materials of elongation at maximum force machine direction (MD)>= 60% and <= 100%, elongation at maximum force (CMD)>= 40%, and  <= 100%, horizontal and vertical permeability (under 2 kn/m2 pressure) = >2×10E-3 m/sec. for effective erosion protection in hydraulic structures / river training works including local handling, placing in position, providing machine seamed joints (with 100% poly prop line or nylon thread) of 35 cm. lap in dry condition or minimum 100 cm lap under water including protecting the geo textile material  from UV ray and from any other damages including with supply of all materials , lobours, equipments etc. complete  as per direction of Engineer in charge.

(Geo textile delivered at site should be certified by ISO and clearly labeled with brand name and grade printed at regular intervals accross the body of the fabric).                    

Mass = > 350gm/m2 , thickness ( Under 2 kpa pressure) = > 2.50 mm, EoS< = 0.09 mm, strip tensile strength = > 20 kn/m, grab strength = > 1200N, CBR puncture resistance = > 3200N.


N.B. The Notice is also available over 

BWDB web site  : www.bwdb.gov.bd  &

CPTU  web site  : www.cptu.gov.bd


All other terms and conditions of the tender will remain unchanged.


This Corrigendum Notice will form part of the Tender Documents.

(Md. Mahbubar Rahman)

Executive Engineer,

Nilphamari O&M Division,

BWDB, Nilphamari.
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