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	BANGLADESH WATER DEVELOPMENT BOARD

Office of the Executive Engineer

Rangpur O&M Division
BWDB, Rangpur.
	    Phone:

0521-63509 (Off)

0521-65593{Res).




Memo no. T-9 /2051 (15)




                    



Date:  12-09-2013 

CORRIGENDUM NOTICE NO. 01

TENDER NO. 03/2013-2014

This is to notify for all concerned that the Tender No.03/2013-2014 invited by the undersigned vide this office Memo. No.T-9/1843(15) dated 19-08-2013, the following new instructions as Corrigendum of tender notice are hereby made due to unavoidable circumstances:

	As Original Tender Notice
	As Corrigendum No.01

	Package No.
	ITT Clause
	Section-2. Tender Data Sheet

(C. Qualification Criteria)
	Package No.
	ITT Clause
	Section-2. Tender Data Sheet

(C. Qualification Criteria)

	RAN-Guti-01
	ITT 7.1
	A satisfactory completion of similar works (i.e. Spur, Groyne & Revetment works) of at least Tk 120.00 lakhs under 1 of contract over a period of last 5 years shall be required. 
	RAN-Guti-01
	ITT 7.1
	A satisfactory completion of similar works (i.e. Spur, Groyne & Revetment works) of at least Tk 87.00 lakhs under 1 of contract over a period of last 5 years shall be required. 

	
	ITT 8.1(a)
	The required average annual construction turnover shall be greater than Tk 170 lakhs over the last 5 years.
	
	ITT 8.1(a)
	The required average annual construction turnover shall be greater than Tk 122.00 lakhs over the last 5 years.

	RAN-Mir-02
	ITT 7.1
	A satisfactory completion of similar works (i.e. Spur, Groyne & Revetment works) of at least Tk 108.00 lakhs under 1 of contract over a period of last 5 years shall be required. 
	RAN-Mir-02
	ITT 7.1
	A satisfactory completion of similar works (i.e. Spur, Groyne & Revetment works) of at least Tk 78.00 lakhs under 1 of contract over a period of last 5 years shall be required. 

	
	ITT 8.1(a)
	The required average annual construction turnover shall be greater than Tk 155 lakhs over the last 5 years.
	
	ITT 8.1(a)
	The required average annual construction turnover shall be greater than Tk 109.00 lakhs over the last 5 years.

	RAN-Rah-03
	ITT 7.1
	A satisfactory completion of similar works (i.e. Spur, Groyne & Revetment works) of at least Tk.119.00 lakhs under 1 of contract over a period of last 5 years shall be required. 
	RAN-Rah-03
	ITT 7.1
	A satisfactory completion of similar works (i.e. Spur, Groyne & Revetment works) of at least Tk.85.50 lakhs under 1 of contract over a period of last 5 years shall be required. 

	
	ITT 8.1(a)
	The required average annual construction turnover shall be greater than Tk 170 lakhs over the last 5 years.
	
	ITT 8.1(a)
	The required average annual construction turnover shall be greater than Tk 119.50 lakhs over the last 5 years.

	Package No.
	Sl. No.

Item Code
	Section-6. Bill of Quantities(BOQ)

Item Description 
	Package No.
	Sl. No.

Item Code
	Section-6. Bill of Quantities(BOQ)

Item Description 

	RAN-Guti-01
	5.
40-140
	Manufacturing and supplying c.c. Blocks in leanest mix. 1:3:6 with cement, sand (FM>=1.5) and shingles (40mm down graded), to attain a minimum 28 days cylinder strength of 9.0 N/mm2 including grading, washing shingles, mixing, laying in forms, consolidation, curing for at least 21 days, including preparation of platform, shuttering and stacking in measurable stacks etc. complete including supply of all materials (steel shutter to be used) as per direction of Engineer in charge.
	RAN-Guti-01
	5.
40-140
	Manufacturing and supplying c.c. Blocks in leanest mix. 1:3:6 with cement, sand (FM>=1.5) and Stone Chips (40mm down graded), to attain a minimum 28 days cylinder strength of 9.0 N/mm2 including grading, washing Stone Chips, mixing, laying in forms, consolidation, curing for at least 21 days, including preparation of platform, shuttering and stacking in measurable stacks etc. complete including supply of all materials (steel shutter to be used) as per direction of Engineer in charge.

	RAN-Mir-02
	5.
40-140
	Manufacturing and supplying c.c. Blocks in leanest mix. 1:3:6 with cement, sand (FM>=1.5) and shingles (40mm down graded), to attain a minimum 28 days cylinder strength of 9.0 N/mm2 including grading, washing shingles, mixing, laying in forms, consolidation, curing for at least 21 days, including preparation of platform, shuttering and stacking in measurable stacks etc. complete including supply of all materials (steel shutter to be used) as per direction of Engineer in charge.
	RAN-Mir-02
	5.
40-140
	Manufacturing and supplying c.c. Blocks in leanest mix. 1:3:6 with cement, sand (FM>=1.5) and Stone Chips (40mm down graded), to attain a minimum 28 days cylinder strength of 9.0 N/mm2 including grading, washing Stone Chips, mixing, laying in forms, consolidation, curing for at least 21 days, including preparation of platform, shuttering and stacking in measurable stacks etc. complete including supply of all materials (steel shutter to be used) as per direction of Engineer in charge.

	RAN-Rah-03
	5.
40-140
	Manufacturing and supplying c.c. Blocks in leanest mix. 1:3:6 with cement, sand (FM>=1.5) and shingles (40mm down graded), to attain a minimum 28 days cylinder strength of 9.0 N/mm2 including grading, washing shingles, mixing, laying in forms, consolidation, curing for at least 21 days, including preparation of platform, shuttering and stacking in measurable stacks etc. complete including supply of all materials (steel shutter to be used) as per direction of Engineer in charge.
	RAN-Rah-03
	5.
40-140
	Manufacturing and supplying c.c. Blocks in leanest mix. 1:3:6 with cement, sand (FM>=1.5) and Stone Chips (40mm down graded), to attain a minimum 28 days cylinder strength of 9.0 N/mm2 including grading, washing Stone Chips, mixing, laying in forms, consolidation, curing for at least 21 days, including preparation of platform, shuttering and stacking in measurable stacks etc. complete including supply of all materials (steel shutter to be used) as per direction of Engineer in charge.


      All other descriptions & terms and conditions of the tender will be remaining unchanged & this corrigendum Notice will be a part of the Tender Document. 

               N.B.This Corrigendum notice will be available in the website of BWDB www.bwdb.gov.bd. And CPTU www.cptu.gov.bd.
 (Md. Abul Kalam Azad) 

Executive Engineer

Rangpur O&M Division

BWDB, Rangpur.
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