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	Office of the Executive Engineer

Dhaka O&M Division-2, hASAN COURT 

(5th Floor), 23/1, Motijheel C/A

Dhaka-1000.  ( 02-7121142
Email: eedhaka2@gmail.com



Memo No: T-3/2272
                                             
               Date: 22-06-2016
Corrigendum No-02 

of 

Tender Notice No-01/2015-16  PACKAGE NO- PANI-01/2015-16

This is for all concerned that the Tender Notice No-01/2015-2016, Package No-PANI-01/2015-16 circulated vide this office Memo No.T-3/2018(50), Dated 19/05/2016 has been amended as following due to unavoidable circumstances:
	BOQ

(Volume-2)
	Existing Provision
	Amended Provision

	Part-A

Item Sl. No-52
	Supplying, fitting and fixing of aluminium curtain wall with aluminium top hung/casement windows as per the US Architectural aluminium Manufacturer's Association (AAMA) Standard Specification having 100 mm , 50mm, 2mm curtain wall sub-mullim outer and inner frame, 15 mm thick casement outer frame (size 38.86 mm 36.6mm), 1.9 mm thick casement shutter (size 47.62mm, 28.57mm,) 1.2 mm thick  shutter glass strips, all aluminium member will be powder coated with coal not less than 1.5 micron in thickness including all accessories 4 bar hinge casement handle, 50 m x 50mm x 6m aluminium angle, steel rowel bolt, screws , rivets norton tape masking tape, structural sealant, gum bracket rod etc. all complete in all respect as per drawing and direction of the Engineer in charge.
	Supplying, fitting and fixing of aluminium curtain wall with aluminium top hung/casement windows as per the US Architectural aluminium Manufacturer's Association (AAMA) Standard Specification having 100 mm , 50mm, 2mm curtain wall sub-mullim outer and inner frame, 1.5 mm thick casement outer frame (size 38.86 mm 36.6mm), 1.9 mm thick casement shutter (size 47.62mm, 28.57mm,) 1.2 mm thick  shutter glass strips, all aluminium member will be powder coated with coal not less than 1.5 micron in thickness including all accessories 4 bar hinge casement handle, 50 m x 50mm x 6m aluminium angle, steel rowel bolt, screws , rivets norton tape masking tape, structural sealant, gum bracket rod etc. all complete in all respect as per drawing and direction of the Engineer in charge.

	Part-B

Item Sl. No-3 (i) to (ix)
	Supplying different inside dia best quality PPR pressure pipe/CPVC Pipe for water supply having specific gravity 1.35 -1.45, and other physical, chemical, thermal, fire resistivity properties etc. as per BSTI approved manufacturer standards or ASTM, BS/ISO/IS standards fitted and fixed in position with sockets, bends, with all accessories such as Round grating/domed roof grating etc. complete approved and accepted by the Engineer-in-charge/ Authority. (length: 6000 mm each).
Item Sl no 3-(i) to 3-(ix)-PPR/CPVC
	Supplying different inside dia best quality CPVC Pipe for water supply having specific gravity 1.35 -1.45, and other physical, chemical, thermal, fire resistivity properties etc. as per BSTI approved manufacturer standards or ASTM, BS/ISO/IS standards fitted and fixed in position with sockets, bends, with all accessories such as Round grating/domed roof grating etc. complete approved and accepted by the Engineer-in-charge/ Authority. (length: 6000 mm each).
Item Sl no 3-(i) to 3-(ix)-CPVC


All other terms & conditions will remain unchanged.

S
(Md. Rafiqul Islam Choubey)

Executive Engineer

Dhaka O&M Division-2

BWDB, Dhaka.
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