Office of the Project Director, Project Management unit, 
Capital (Pilot) Dredging of the River System in Bangladesh, BWDB, Dhaka
Addendum to the Prequalification Document No: CDRSB/PQ-01/2010-2011 for Capital (Pilot) Dredging of River Jamuma 

Addendum No.02
Following amendments are made in the Prequalification Document No: CDRSB/PQ-01/2010-2011 for Capital (Pilot) Dredging of River Jamuna invited by Project Director, Project Management unit, Capital (Pilot) Dredging of the River System in Bangladesh, BWDB, Dhaka , vide his memo no. PD/PMU-CDRSB/T-1/11   Date: 04/11/2010:
i
The name and total length of river to be dredged under the Prequalification invitation is amended as follows:
	Prequalification Notice Sl No. 
	Proposed Tender Package Name and length as per Prequalification Notice
	Proposed Tender Package Name and length as per Prequalification Notice as per amendments



	15
	Dredging of the River Jamuna (1st year Capital Dredging and 2nd year maintenance dredging)  with ancillary works from Sirajganj Hard Point to Dhaleswari Offtake ( 20 Km )


	Dredging of the River Jamuna (1st year Capital Dredging and 2nd year maintenance dredging)  with ancillary works from Sirajganj Hard Point to near Bangobandhu Bridge 
( 14Km )


ii
Identifications of lot and location as specified in Sl No.26 of Prequalification Notice are amended as follows: 
	Prequalification Notice Sl No.
	Lot No.
	As per Prequalification Notice
	As per amendments

	
	
	Identification of Lot
	Location
	Identification of Lot
	Location

	26
	01
	From Km.0.000 to Km.10.000


	Upazila:Sirajganj Sadar, Dist: Sirajgang
	From Km.0.000 to Km.7.000


	Upazila:Sirajganj Sadar, Dist: Sirajgang

	
	02
	From Km.10.000 to Km.20.000


	Upazila:Sirajganj Sadar, Bhuapur and Kalihati, Dist: Sirajgang an Tangail
	From Km.7.000 to Km.14.000

	Upazila:Sirajganj Sadar and Bhuapur, Dist: Sirajgang an Tangail


iii
Consequently ITA 1.1, Page 21 : Brief Description of the Works and size of lot are amended as follow:
	Clause No

Page No.
	Brief Description of the Works and size of lot as per prequalification Document
	Brief Description of the Works and size of lot as per amendments



	ITA 1.1
21
	The works comprise dredging of Jamuna River from Sirajganj Hard Point to Dhaleswari Offtake for a length of 20 Km to divert the river flow from east channel into mid channel and thereby reduce the risk of failure of Sirajganj hard point. It also aimed at guiding the flow along the mid section of existing char through Bangobandhu Bridge to near Dhaleswari Offtake. It will reduce the risk of riverbed scour along the Sirajganj Hard Point and lessen erosion of right Guide Bundh of Bangobandhu Bridge. The works also include transportation and safe disposal of the dredged spoil up to a distance of 3000 metre at the specified area as are shown in the related drawings or as directed by the Engineer in conformation to the specifications.
Lot No(s):

Lot No.1 :  From Km.0.000 to Km.10.000

Lot No.2 :  From Km.10.000 to Km.20.000
	The works comprise dredging of Jamuna River from Sirajganj Hard Point to near Bangobandhu Bridge for a length of 14 Km to divert the river flow from east channel into mid channel and thereby reduce the risk of failure of Sirajganj hard point. It also aimed at guiding the flow along the mid section of existing char through Bangobandhu Bridge to near Dhaleswari Offtake. It will reduce the risk of riverbed scour along the Sirajganj Hard Point and lessen erosion of right Guide Bundh of Bangobandhu Bridge. The works also include transportation and safe disposal of the dredged spoil up to a distance of 3000 metre at the specified area as are shown in the related drawings or as directed by the Engineer in conformation to the specifications.
Lot No(s):

Lot No.1 :  From Km.0.000 to Km.7.000

Lot No.2 :  From Km.7.000 to Km.14.000


iv
Following Clauses of Qualification Criteria are also amended  :
	Clause No.

Page No
	Qualification requirements  as per Tender document

	Qualification requirements as per amendments


	ITA 14.1(c)
22

	A satisfactory completion of following similar works as a Prime Contractor or Subcontractor or as a partner of Joint Venture over a period of 10(ten) years shall be required.
a) One project of River/Channel dredging of minimum Contract value of BDT 2700.00 million ie  USD 39.00  million equivalent in a single contract

b)   One project of dredging of dredged volume 10.8 million M3 or more in a  single contract
( above qualification requirements are  applicable  for each of the lots in the package)
	A satisfactory completion of following similar works as a Prime Contractor or Subcontractor or as a partner of Joint Venture over a period of 10(ten) years shall be required.
a) One project of River/Channel dredging of minimum Contract value of BDT 1890.00 million ie  USD 27.39  million equivalent in a single contract

b)   One project of dredging of dredged volume 7.6 million M3 or more in a  single contract

( above qualification requirements are  applicable  for each of the lots in the package)

	ITA 15.1(a)

23


	The required average annual construction turnover shall be greater than BDT 2375.00 million i.e. USD 49.00 million equivalent over the last 5(five) years.

( above qualification requirements are  applicable  for each of the lots in the package)
	The required average annual construction turnover shall be greater than BDT 2363.00 million i.e. USD 34.24 million equivalent over the last 5(five) years.

( above qualification requirements are  applicable  for each of the lots in the package)

	ITA 15.1(b)

23
	The minimum Tender Capacity shall be: BDT 3150.00 million i.e. USD 46.00 million equivalents.
( above qualification requirements are  applicable  for each of the lots in the package)
	The minimum Tender Capacity shall be: BDT 2205.00 million i.e. USD 31.96 million equivalents.
( above qualification requirements are  applicable  for each of the lots in the package)

	ITA 15.1(c)

23
	The minimum amount of liquid assets or working capital or credit facilities of the Applicant shall be BDT 1438.00 million i.e .USD 21.00 million equivalents.
( above qualification requirements are  applicable  for each of the lots in the package)
	The minimum amount of liquid assets or working capital or credit facilities of the Applicant shall be BDT 1008.00 million i.e .USD 14.61 million equivalents.
( above qualification requirements are  applicable  for each of the lots in the package)

	ITA 17.1

24 & 25
	The Applicant shall own or have proven access to hire or lease of the major construction  equipments, in full working order as follows :

Name of Equipment

Minimum Numbers required

Specification/Capacity of
 Equipment

Minimum
Requirement
Dredger 

Cutter Suction Dredger 

05

Dredge Pump=1910 KW

Suction Pipe= 686 mm
dia

Discharge Pipe=610
 mm  dia

Sludge Discharge= 

Minimum 900 m3/hour at
 discharge point of
 about  3000 metre 
Ancillary Equipment 
Work boat /crane boat for fitting fixing of discharge pipe line and preparation of dredging

04

Compatible to the
 dredgers as specified  

Tug Boat

04

1000 HP

Survey vessel

02

To be equipped with
 RTK GPS , Eco-
sounder, Laptop with 
related software(Hydro 
or recently available), 
plotter  and other 
accessories to carry 
out bathymetric survey
 and production of in 
situ cross-section of 
river bed  

Dry Earth Equipment

Excavator/
Dragline

4

With the capacity to
 assist in spoil 
management

Bull Dozer

4

-do-

( above qualification requirements are  applicable  for each of the lots in the package)
	The Applicant shall own or have proven access to hire or lease of the major construction  equipments, in full working order as follows as per amendments :
Name of Equipment

Minimum Numbers required

Specification/Capacity of Equipment

Minimum Requirement

Dredger 

Cutter Suction Dredger 

04
Dredge Pump=1910 KW

Suction Pipe= 686 mm dia

Discharge Pipe=610 mm dia

Sludge Discharge= Minimum 900 m3/hour at  discharge point of about  3000 metre 
Ancillary Equipment 
Work boat /crane boat for fitting fixing of discharge pipe line and preparation of dredging

03
Compatible to the dredgers as specified  

Tug Boat

03
1000 HP

Survey vessel

02

To be equipped with RTK GPS , Eco-sounder, Laptop with related software (Hydro or recently available), plotter  and other accessories to carry out bathymetric survey and production of in situ cross-section of river bed 
Dry Earth Equipment

Excavator/
Dragline

3
With the capacity to assist in spoil management
Bull Dozer

3
-do-

( above qualification requirements are  applicable  for each of the lots in the package)


v
Total volume of dredging in each lot as specified in Section-4, Scope of Works, under “Description of works” in Para 4, 2nd  & 3rd line, Page No.42 is corrected as follows;
	Page No
	Total volume of dredging in each lot as Prequalification Document
	Total volume of dredging in each lot as per amendments

	42
	to the tune of 18 million metre cube( capital-11.5  million metre cube and maintenance 6.5 million metre cube)  
	to the tune of 12.6 million metre cube( capital-8.1  million metre cube and maintenance 4.5 million metre cube)  


vi
Caption of 3rd Column in Sl.iii of Addendum No.01 issued vide Memo No. PD/PMU-CDRSB/T-1/064 dated 14-12-2010 is corrected as “Last Date of Selling of the Prequalification Document as per amendments” instead of “Opening of the Tenders as per amendments”
All other terms and conditions and contents of the Prequalification Document will remain unchanged. 

This Addendum shall form an integral part of the Prequalification Document pursuant to ITA Clause No.11.2








Sd\-

((Jati Das Kundu)

                                              Project Director
                                                  
                                                          Project Management unit
                                             Capital (Pilot) Dredging of the River                                                            System in Bangladesh
                                                                                                  BWDB, Dhaka
Memo No. PD/PMU-CDRSB/T-1/088
                              Dated 04-01-2011
Copy for favour of kind information/ information and wide circulation to:
01 The Director General, C.P.T.U, Planning Commission, Block-12 (2nd floor), Sher-E-Bangla Nagar, Dhaka.

02 The Additional Director General, O&M-East Region, BWDB, Dhaka
03 The Additional Director General, O&M-West Region, BWDB, Dhaka
04-05         The Chief Engineer, North Western Zone/Central Zone, BWDB, Rajshahi / Dhaka 

O6
The Director, Contract & Procurement Cell, BWDB, Dhaka, WAPDA BHABAN,( 9th Floor), Motijheel, C/A, Dhaka

07-08         The Superintending Engineer, Bogra / Mymensingh O&M Circle, BWDB, Bogra/ Mymensingh 

09-10         The Deputy Commissioner Serajgonj/Tangail

11-12         The Executive Engineer, Serajgonj/ Tangail O & M Division, BWDB,  Serajgonj/ Tangail.

 13          System Analyst, Computer Section, Chief Monitoring Office, WAPDA BHABAN,( 3rd Floor), Motijheel,  C/A, Dhaka. He is requested to arrange all necessary action to publish the Addendum   in website of C.P.T.U and BWDB (CD enclosed)

014           The Account Officer, Regional Accounting Centre (RAC), Green Road, BWDB, Dhaka
015    The Manager, Janata Bank Ltd. 29 Dilkhusha Corporate Branch, Dilkhusha C/A Dhaka-1000.    ………..No Addendum No.02 are for sent herewith for attaching with the unsold Prequalification Document before being sold to the intending Applicants up to banking hours on 19-01-2011.

16
Notice Board

17
Mr./Mrs………………………………………………………………………………………… He/they is/are requested to acknowledge the receipt of the Addendum (No.2) within 3(three) working days.

(Jati Das Kundu)
                                              Project Director
                                                                                                            Project Management unit
                                             Capital (Pilot) Dredging of the River                                                            System in Bangladesh
                                                                                                  BWDB, Dhaka
