Office of the Executive Engineer

Tangail O & M Division

BWDB, Tangail
Addendum to the Tender Document No: 04/2010-2011
 for Dredging of River Jamuna from upstream of Bangobandhu Bridge to Dhaleswari Offtake in Upazila: Bhuapur and Kalihati,   Dist: Tangail( 6 km )
Addendum No.01
Following amendments are made in the Tender Document No: 04/2010-2011, Package No.CDRSB-BHU & KAL/Tang-04 for Dredging of River Jamuna from upstream of Bangobandhu Bridge to Dhaleswari Offtake in Upazila: Bhuapur and Kalihati,   Dist: Tangail ( 6 km ) invited by the Executive Engineer, Tangail O & M Division , vide his memo no. T-6/1340 date 26-01-2011;
i
ITT 42.1, Page 33: The deadline of submission of the Tender is extended as follows:

	Clause No

Page No.
	The deadline of submission of the Tender as per Original Document
: Time & Date
	The deadline of submission of the Tender as per amendments

: Time & Date

	ITT 42.1
33
	1200 hours , 07 March,2011
	1200 hours , 21 March, 2011


ii
Consequently ITT 48.1, Page 33 : Time and Date of tender opening is amended as follow:

	Clause No

Page No.
	Opening of the Tenders as per Original Document
: Time & Date
	Opening of the Tenders as per amendments

: Time & Date

	ITT 48.1
33
	1300 hours , 07 March,2011
	1400 hours , 21 March,2011


iii
Last Date of Selling of the Tenders also extended as follows:

	Tender Notice Sl No.
	Last Date of Selling of the Tender  Document as per Notice

: Time & Date
	Last Date of Selling of the Tenders as per amendments

: Time & Date

	15
	Up to 06 March, 2010
	Up to 20 March, 2011


iv
Following Clause of Qualification Criteria is amended : 
	ITT No

Page No
	Requirements as the original Tender Document
	Requirements as per amendment

	ITT No.17.1
No.30 & 31
	The Tenderer shall own 2 nos Dredger and have proven access to own/ hire or lease another dredger and own of the major construction  equipments, in full working order as follows :

Name of Equipment

Minimum Numbers required

Specification/Capacity of Equipment

Minimum

 Requirement

Dredger 

a.Cutter Suction Dredger 

02

(The Tenderer shall own 2 nos Dredger)
Dredge Pump=620 KW

Suction Pipe= 450 mm dia, 

Discharge Pipe=450 mm dia, 

minimum 4,000.00 m in length

Sludge Discharge= Minimum

 400 m3/hour at  an average 

discharge points  of about  3000 m
b. Cutter Suction Dredger

01

(have proven access

to own / hire or lease

another dredger
Dredge Pump=620 KW

Suction Pipe= 450 mm dia, 

Discharge Pipe=450 mm dia, 

Sludge Discharge= Minimum

 400 m3/hour at  an average 

discharge points  of about  3000 m

Ancillary Equipment 
Work boat /crane boat for fitting fixing of discharge pipe line and preparation of dredging
02
Compatible to the

 dredgers as specified  

Tug Boat

02
1000 HP

Survey vessel

01
To be equipped with  RTK 
GPS , Eco-sounder, Laptop with 
related software(Hydro or recently 
available), plotter  and other 

accessories to carry out bathymetric
 survey and production of in situ
 cross-section of river bed  
Dry Earth Equipment

Excavator/

Dragline

2
With the capacity to

 assist in spoil 

management

Crawler Tractor
4

240 HP
Vibratory Compactor

3

43 HP

( above qualification requirements are  applicable  for each of the lots in the package)
	The Tenderer shall own 2 nos/01 Nos Dredger and have proven access to own/ hire or lease another dredger and own of the major construction  equipments, in full working order as follows  as per :

Name of Equipment

Minimum Numbers required

Specification/Capacity 
of Equipment

Minimum Requirement

Dredger 

a.Cutter Suction Dredger 

02

(The Tenderer shall own 2 nos Dredger)
Or

01

(The Tenderer shall own 1 nos Dredger)

Dredge Pump=620 KW

Suction Pipe= 450 mm dia, 

Discharge Pipe=450 mm dia, minimum 4,000.00 m in length

Sludge Discharge= Minimum 400 m3/hour at  an average discharge points of about  3000 m
Dredge Pump=1910 KW

Suction Pipe= 686 mm dia

Discharge Pipe=610 mm dia, minimum 4,000.00 m in length 
Sludge Discharge= Minimum 900 m3/hour at   an average discharge points of 3000 m
b. Cutter Suction Dredger
01

      (have proven access

  to own / hire or lease

another dredger
Dredge Pump=620 KW

Suction Pipe= 450 mm dia, 

Discharge Pipe=450 mm dia, 

Sludge Discharge= Minimum

 400 m3/hour at  an average 

discharge points  of about  3000 m

Ancillary Equipment 
Work boat /crane boat for fitting fixing of discharge pipe line and preparation of dredging

02
Compatible to the dredgers as specified  

Tug Boat

02
1000 HP

Survey vessel

01

To be equipped with RTK

GPS , Eco-sounder, Laptop with related software

 (Hydro or recently available), plotter  and other accessories to carry out bathymetric survey and production of in situ cross-section of river bed 

Dry Earth Equipment

Excavator/

Dragline

3

With the capacity to assist in spoil management

Crawler Tractor
3

-do-

Vibratory Compactor

3

43 HP

( above qualification requirements are  applicable  for each of the lots in the package)


v
The Defect Liability Period as specified in GCC 57.1 is amended as follows:

	Clause No

Page No.
	The Defect Liability Period as per Original Document
	The Defect Liability Period as per amendments



	GCC 57.1

69
	12 (twelve) months 
	a) For Dredged Channel : 0 (zero) month
b) For disposed earth     : 06 (six) months


All other terms and conditions and contents of the Tender Document will remain unchanged. 

This Addendum shall form an integral part of the Tender Document pursuant to ITA Clause No.11.2








Sd\-

(I.M.REAZUL HASAN)

   Executive Engineer

  Tangail O&M Division 

     BWDB, Tangail
Memo No.T6/1526(40)
                              Dated 24-02-2011
Copy for favour of kind information/ information and wide circulation to:
01 The Director General, C.P.T.U, Planning Commission, Block-12 (2nd floor) , Sher-E-Bangla Nagar, Dhaka.

02 The Additional Director General, East Region, BWDB, Dhaka
03 The Additional Director General, West region , BWDB, Dhaka
04 The Chief Engineer, Central Zone, BWDB, Dhaka ( Copy of Addendum No.01 is  enclosed)

05 The Project Director, Project Management Unit, Capital (Pilot) Dredging of River System in Bangladesh,     72, Green Road, Dhaka. He is requested to please be present himself or depute one representative from his office to remain present on the day of submission till opening of the Tenders.

06 The Metropolitan Police Commissioner of Dhaka (DMP). He is requested to please provide all kind of security on the amended date on  21-03-2011 at the Office of the Project Director, Project Management Unit, Capital (Pilot) Dredging of River system in Bangladesh, 72, Green Road, Dhaka in c/w the tender process.

07 The Director, Contract & Procurement Cell, BWDB, Dhaka, WAPDA BHABAN,( 9th Floor), Motijheel, C/A, Dhaka

08 The Superintending Engineer, Mymensingh O&M Circle, BWDB, Mymensingh (Copy of Addendum No.01 is enclosed).

09 The Deputy Commissioner Tangail

10-12 The Executive Engineer, Mymensingh/ Jamalpur/ Netrakona O & M Division, BWDB,  Mymensingh /Jamalpur /Netrakona

13 The Executive Engineer, Keshoreganj WD Division, BWDB, Kishoreganj

14-16 The Executive Engineer, LGED/PWD/R&H, Tangail

17 System Analyst, Computer Section, Chief Monitoring Office, WAPDA BHABAN,( 3rd Floor), Motijheel, C/A, Dhaka. He is requested to arrange all necessary action to publish the Addendum No.01  in website of C.P.T.U (CD enclosed)

18 The Account Officer, Regional Accounting Centre (RAC), BWDB, Mymensingh

19-20 The Sub-Divisional Engineer, Tangail O & M Sub-Division-1/2 BWDB, Tangail

21-22 The Upazila Nirbahi Officer, Bhuapur/Kalihati in the District of Tangail

23 The Manager, Janata Bank Ltd. 29 Dilkhusha Corporate Branch, Dilkhusha C/A Dhaka-1000. …………copies Addendum No.01 are sent herewith for attaching with the unsold Tender Document before being sold to the intending Tenderers up to banking hours on 20/03/2010
24-25 Estimator/Asstt. Accountant/ Head Asstt. Of this Division

26
Notice Board

27
Mr./Mrs…………………………………………………………………………………………..





(I.M.REAZUL HASAN)

   Executive Engineer

  Tangail O&M Division 

       BWDB, Tangail
