Office of the Executive Engineer
Tangail O & M Division

BWDB, Tangail
INVITATION FOR FRESH TENDER

TENDER NO.06/2010-2011
	GOVERNMENT OF THE PEOPLE’S REPUBLIC OF BANGLADESH

	1
	Ministry/Division
	Ministry of Water Resources

	2
	Agency
	Bangladesh Water Development Board

	3
	Procuring Entity Name
	Project Director, Project Management Unit

Capital(Pilot) Dredging of River System in Bangladesh 

	4
	Procuring Entity District
	Dhaka

	5
	Invitation for 
	Capital Dredging (Works) 

	6
	Invitation Ref No
	T-6/2408

	7
	Date
	09-06-11

	KEY INFORMATION

	8
	Procurement Method
	NCT Open Tendering Method (National)

	FUNDING INFORMATION

	9
	Budget and Source of Funds
	Development Budget GoB

	10
	Development Partners (if applicable)
	None

	PARTICULAR INFORMATION

	11
	Project Name 
	Capital(Pilot) Dredging of  River System in Bangladesh 

	12
	Tender Package No.
	CDRSB-BHU & KAL/Tang-06

	13
	Tender Package Name
	Dredging of River Jamuna from Upstream of Bangabandhu Bridge to Dhaleswari Offtake for a total length maximum 6.00 Km, Upazila: Bhuapur & Kalihati, Dist: Tangail

	14
	Tender Publication Date
	09-06-11

	15
	Tender Last Selling Date
	25-07-11

	
	
	Date
	Time

	16
	Tender Closing Date and Time
	26-07-11
	1200

	17
	Tender Opening Date and Time
	26-07-11
	1400

	18
	Name & Address of the office(s)
	

	
	- Selling Tender Document (Principal)
	Manager, Janata Bank Ltd. Dilkhusha Corporate Branch

Address: 29, Dilkhusha Commercial Area, Dhaka-1000

Telephone No.: 88-02-9554136, PABX-88-02-9560058-59

Fax No.:88-02-9551783

e-mail address: jbdil@janatabank-bd.com,  jbdcbfex@yahoo.com

	
	- Selling Tender Document (Others)
	None

	
	NO CONDITIONS APPLY FOR SALE , PURCHASE OR DISTRIBUTION OF TENDER DOCUMENTS

	
	- Receiving Tender Document
	Office of the Project Director , Capital (Pilot) Dredging of River System in Bangladesh, BWDB, 72 Green Road , Dhaka

	
	- Opening Tender Document
	Office of the Project Director , Capital (Pilot) Dredging of River System in Bangladesh, BWDB, 72 Green Road , Dhaka

	19
	Place / Date / Time of 
	BWDB’s Conference Room, WAPDA BHABAN (3rd floor), Motijheel C/A,Dhaka

	
	Pre-Tender Meeting 
	Date
	04-07-11
	Time
	1500 hrs

	INFORMATION FOR TENDERER

	20
	Eligibility of Tenderer    
	This Invitation for Tenders is open to all potential Tenderers having 

a) Minimum 5 (five) years period of general experience in the      construction works/dredging works and Minimum Annual Average Construction Turnover in the last 5 (five) years preceding the date of submission of tender is not less than BDT 621.00 million for      Lot-01, BDT 409.00 million for Lot-02 & BDT 534.00 million for Lot-03. This requirement is exempted for the Bangladeshi Farm/Tenderer who own at least 1(one) 450 mm Cutter Section Dredger .
b) The minimum amount of liquid assets or working capital or credit facilities of the  Tenderer shall be BDT 177.00 million for Lot-01, BDT 117.00 million for Lot-02 & BDT 153.00 million for Lot-03
c) i) Minimum specific experience as a Prime Contractor or Subcontractor or Partner in Joint Venture in Construction works of at least 1(one) contract of similar nature, complexity of dredging works successfully completed in the last 5(five) years with contract value at least BDT 414.0 million for Lot-01, BDT 273.00 million for Lot-02, and BDT 356.00 million for Lot-03. This requirement is exempted for the Bangladeshi Firm/ Tenderer who own at least 1(one) 450 mm Cutter Section Dredger.
ii)   The required average annual construction turnover shall be greater than BDT 621.00 million for Lot-01 , BDT 409.00 million for Lot-02 & BDT 534.00 million for Lot-0-3  over the last 5 (five) years. This requirement is exempted for the Bangladeshi Firm/ Tenderer who own at least 1(one) 450 mm Cutter Section Dredger.
 iii)   The Tenderer  must  own minimum of 2(two) Nos 450 mm dia Cutter Suction Dredger with a Sludge Discharging Capacity Minimum 400 m3/hour at an average distance of 3000 m or   1(one) No 600 mm Cutter Suction Dredger  with a Sludge Discharging Capacity Minimum 900 m3/hour at an average distance of 3000 m 

iv)    have proven access to hire or lease minimum of 1(one) No. 450 mm dia Cutter Suction Dredger with a Sludge Discharging Capacity of Minimum 400 m3/hour  at an average distance of 3000 m. and

v)  Other requisite equipment capabilities as specified in Tender   Data Sheet (TDS) and

d) other qualification requirements as specified in Tender Data Sheet (TDS) of the  Tender Document
Attested copies of all necessary supporting documents shall have to be submitted along with the tender.

The prospective Tenderer(s) having experiences outside  Bangladesh in the Construction works as stated above and stipulated in the TDS, , his/their  experience certificate(s) shall have to be got authenticated by his/their country’s Ambassador /High Commissioner in Bangladesh

	21
	Brief Description of  Works
	The works to be done under the Contracts are dredging of Jamuna River from upstream of Bangabandhu Bridge to Dhaleswari Offtake for a length of 6 Km (which may vary in the final run of model with post monsoon bathymetric survey of 2011) to divert the river flow along the mid section of existing char through Bangabandhu Bridge to near Dhaleswari Offtake. The work is aimed at streamlining the river flow through defined channels which in turn will reduce the risk of riverbed scour and lessen erosion of left Guide Bundh of Bangabandhu Bridge. 

The works also include transportation and safe disposal of the dredged spoil up to a distance of 3000 metre at the specified area as are shown in the related drawings or as directed by the Engineer in conformation to the specifications. Management of dredged spoil in proper way and its maintenance for at least 1(one) year is one of main objective of the Dredging. The disposal of dredged spoil is aimed at attainment of land reclamation to be used for future development, like housing settlement, business centre, agriculture farm, industries etc. The disposed/reclaimed area are to be protected from being washed out/eroded away by river current /rain water flow or by any other means with bamboo/bullah piling , dumping/placing geo-bags and synthetic bags, geo fabric sheeting etc.   as per drawing which will be  furnished at the time of issuing Work Order.

The alignment and length of dredging as shown in the Index Map is an indicative one that has been predicted on the basis of model study of pre-monsoon bathymetric data. Final alignment and length of dredging will be predicted after the final run of model study with the post monsoon bathymetric survey. So, the length shown against each Lot is subjected to change depending on the result of model study with the post monsoon bathymetric survey which (length and chainages) will be finalized before issuing the Work Order.   
The entire dredging work under the Package is divided in 3(three) lots, each Lot having a 2 Km segment as shown herein under. 

Volume of capital dredging will be to the tune of 2.12 million M3 , 1.40 million M3 and 1.93 million M3 in Lot-01, Lot-02 and Lot-03 respectively to be accomplished in 1st year followed by maintenance dredging of about 1.19 million M3, 0.78 million M3 and 1.08 million M3 in Lot-01, Lot-02 and Lot-03 respectively to be carried out in the 2nd year. The volumes for both Capital and Maintenance Dredging in all the 3(three) lots are changeable depending upon final run of the Model with post monsoon bathymetric survey data.


	22
	Brief Description of Physical Services
	N/A

	23
	Price of Tender Document 
	i) Lot-01: Tk.15,000/00 (Taka fifteen thousands only)

ii) Lot-02: Tk.15,000/00 (Taka fifteen thousands only)

iii) Lot-03: Tk.15.000/00 (Taka fifteen thousands only)

	24
	Lot No
	Identification of Lot
	Location
	Tender Security
Amount (Tk)


	Completion Time in Weeks / Months

	
	Lot -01
	Dredging of River Jamuna of Maximum length  2.000 Km at  Upstream          

(length and chainages will be finalised  before issuing Work Order depending on the Final Model run with Post monsoon bathymetric of 2011)
	Upazila:Bhuapur, 

Dist: Tangail
	Tk.2,07,00,000.00 (Taka two crore seven lacs only)
	21(Twenty one ) months

	
	Lot -02
	Dredging of River Jamuna of Maximum length  2.000 Km at  mid portion          

(length and chainages will be finalised  before issuing Work Order depending on the Final Model run with Post monsoon bathymetric of 2011)
	Upazila:Bhuapur &  

Kalihati

Dist: Tangail
	Tk.1,36,00,000.00 (Taka one crore thirty six lacs  only)
	21(Twenty one) months

	
	Lot -03
	Dredging of River Jamuna of Maximum length  2.000 Km at  Down Stream        

(length and chainages will be finalised  before issuing Work Order depending on the Final Model run with Post monsoon bathymetric of 2011)
	Upazila:Kalihati, 

Dist: Tangail
	Tk.1,78,00,000.00 (Taka one crore seventy eight lacs only)
	21(Twenty one) months

	PROCURING ENTITY DETAILS:

	25
	Name of Official Inviting Tender
	I.M. Reazul Hasan 

	26
	Designation of Official Inviting Tender
	Executive Engineer

	27
	Address of Official Inviting Tender
	Tangail O&M Division, BWDB, Tangail

	28
	Contact details of Official Inviting Tender
	0921-53401
	Fax-0921-53401
	Reazul58@hotmail.com

	29
	The Procuring Entity reserves the right to reject  all the Tenders or annul the Tender proceedings


( I.M.REAZUL HASAN )

   Executive Engineer

  Tangail O&M Division 

      BWDB, Tangail
Memo No.T-6/2408(40)


Dated 09-06-2011
Copy for favour of kind information/ information and wide circulation to :

01 The Director General, C.P.T.U, Planning Commission, Block-12 (2nd floor), Sher-E-Bangla Nagar, Dhaka.

02 The Additional Director General, East Region, BWDB, Dhaka
03 The Additional Director General, West region , BWDB, Dhaka
04 The Chief Engineer, Central Zone, BWDB, Dhaka ( Copy of Tender Document enclosed)

05 The Project Director, Project Management Unit, Capital (Pilot) Dredging of River System in Bangladesh, 72, Green Road, Dhaka. He is requested to please be present himself or depute one representative from his office to remain present on the day of submission till opening of the Tenders.

06 The Metropolitan Police Commissioner of Dhaka (DMP). He is requested to please provide all kind of security on 26-07-2011 at the Office of the Project Director, Project Management Unit, Capital (Pilot) Dredging of River system in Bangladesh, 72, Green Road, Dhaka in c/w the tender process.

07 The Director, Contract & Procurement Cell, BWDB, Dhaka, WAPDA BHABAN,( 9th Floor), Motijheel, C/A, Dhaka

08 The Superintending Engineer, Mymensingh O&M Circle, BWDB, Mymensingh (Copy of Tender Document enclosed).

09 The Deputy Commissioner Tangail

10-12 The Executive Engineer, Mymensingh/ Jamalpur/ Netrakona O & M Division, BWDB,  Mymensingh /Jamalpur /Netrakona

13 The Executive Engineer, Keshoreganj/Tangail WD Division, BWDB, Kishoreganj/Tangail
14-16 The Executive Engineer, LGED/PWD/R&H, Tangail

17 System Analyst, Computer Section, Chief Monitoring Office, WAPDA BHABAN,( 3rd Floor), Motijheel, C/A, Dhaka. He is requested to arrange all necessary action to publish the Tender Notice  in website of C.P.T.U (CD enclosed)

18 The Account Officer, Regional Accounting Centre (RAC), BWDB, Mymensingh

19-20 The Sub-Divisional Engineer, Tangail O & M Sub-Division-1/2 BWDB, Tangail

21-22            The Upazila Nirbahi Officer, Bhuapur/Kalihati in the District of Tangail

23 The Manager, Janata Bank Ltd. 29 Dilkhusha Corporate Branch, Dilkhusha C/A Dhaka-1000 along with 10(ten) sets of each Lot, Total 30(thirty) sets Tender Document are sent herewith for selling to the intending Tenderers at the rate set forth in the Tender Notice up to banking hours on 25-07-2011.The sale proceeds should be deposited to the STD Account No.36001008 of Janata Bank Ltd. 29 Dilkhusha Corporate Branch, Dilkhusha C/A Dhaka-1000. Unsold Tender Document along with the copy of Credit Advice may please be sent to the undersigned at an earliest

24-25            Estimator/Asstt. Accountant/ Head Asstt. Of this Division

26
Notice Board

27
Mr./Mrs…………………………………………………………………………………………..





(I.M.REAZUL HASAN)

   Executive Engineer

  Tangail O&M Division 

       BWDB, Tangail
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