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	Office of the Executive Engineer

Kishoreganj WD Division

BWDB, Kishoreganj.

Phone: 0941-61842

	BANGLADESH WATER DEVELOPMENT BOARD


ÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑÑ
Memo No. T-1/1421                                                                                                 Date: 21-09-2011                                               

CORRIGENDUM NO. 01 
OF

TENDER NO. 04/2011-12

This is to inform all concerned that the Tender No. 04/2011-12 in connection with Package- KKRMP-01 (DPP-K-W-5), KKRMP-02 (DPP-K-W-12), KKRMP-03 (DPP-K-W-13 & K-W-14), KKRMP-04 (DPP-K-W-15) circulated vide this Office Memo No. T-1/1365 dated: 21-08-2011 has been amended as following due to unavoidable circumstances.  
	TDS Location
	Original / Previous
(Specification/Capacity/Equipment Minimum required)
	Amended 
(Specification/Capacity/Equipment Minimum required)

	Section-2: 

ITT Clause 17.1 *A. Dredger: 

Cutter Suction Dredger’s Specification stated in TDS: 

for both hire and own

	Dredger Pumps=620 KW

Suction Pump=450 mm dia,

Discharge Pipe=450 mm dia, minimum 4000.00 m in length

Sludge Discharge=Minimum 800 m3/hr or more at an average discharge points of about 3000 m
	Dredger Pumps=620 KW

Suction Pump=450 mm dia,

Discharge Pipe=450 mm dia, minimum 3000.00 m in length

Sludge Discharge=Minimum 400 m3/hr or more at an average discharge points of about 3000 m

	
	
	


All other terms and conditions will remain unchanged. This amendment will be the part of this contract. 
Signed/-
21/09/2011

 (Khushi Mohan Sarker)

Executive Engineer

Kishoreganj WD Division

BWDB, Kishoreganj
_1215935167

