Minutes of Pre-Tender Meeting of Tender No. 02/2011-12 in C/W Package No. KKRMP-G-01 & KKRMP-G-02 of “Kalni-Kushiyara River Management Project” under Kishoreganj WD Division during the year 2011-12.
A Pre-Tender meeting in connection with the tender notice no. 02/2011-12 under Kishoreganj WD Division and packages stated above was held on 20th September 2011 at 12-30 hours as per provision of the tender documents in the office room of the Project Director, “Kalni-Kushiyara River Management Project” & Chief Engineer, Central Zone, BWDB, Dhaka. The Project Director “Kalni-Kushiyara River Management Project” and Chief Engineer, Central Zone Chaired the meeting. List of the participants of the meeting is given in the appendix-I.
Welcoming the participants the Chairman explained the main conception of the “Kalni-Kushiyara River Management Project”. He informed that present Government has given the highest priority for implementation of the said project and requested the participants whether they have any question regarding of the Tender Documents. He also outlined the specifications of the equipments (supplying of Long Boom and Standard Excavators) as well. The suggestion of the tenderer and decisions of the meeting are given below: 

	Sl. No.
	Field of Discussion
	Suggestion of Tenderer
	Decision

	01.
	Section-4: GCC Clause 27.3

Payments shall be made in no case later than the days 180 days after submission of an invoice or request for payment by the Supplier, and after the procuring Entity has accepted it. 
	Section-4: GCC Clause 27.3
a) Work order will be issued after getting clearance from the competent authority. 

b) Payment will be made on the basis of fund availability. 
	Section-4: GCC Clause 27.3
a) Work order will be issued after getting clearance from the competent authority. 

b) Payment will be made on the basis of fund availability and no claim in this regard will be entertained. 

	02.
	Technical Specification: 

1.14 Mandatory Spare Parts

a) Ditch cleaning bucket (without teeth)-1 set;

b) Ditch cleaning bucket (with teeth)-1 set;

c) Swing gear pinion system-2 set;

d) Hydraulic hose pipe (different size as required)-2 set (10 nos);

e) Panel Board-1 set;

f) Bucket tooth accessories-6 sets;

g) Major over hulling kits for engines and hydraulic pumps-1 set;

h) Hydraulic pump complete-1 set;

i) Fuel pump complete-1 set.
	Technical Specification: 

1.14 Mandatory Spare Parts

a) Fuel filter primary – 15 nos;

b) Fuel filter secondary- 15 nos;

c) Oil filter – 15 nos;

d) Hydraulic filter - 5 nos;

e) Air filter – 5 nos;

f) Ditch cleaning bucket (with teeth) – 1 set;

g)Hydraulic hose pipe (Different sizes) – 2 set (10 nos);

h) Panel board – 1 set.


	Technical Specification: 

1.14 Mandatory Spare Parts

a) Fuel filter primary – 15 nos;

b) Fuel filter secondary- 15 nos;

c) Oil filter – 15 nos;

d) Hydraulic filter - 5 nos;

e) Air filter – 5 nos;

f) Ditch cleaning bucket 
(with teeth) – 1 set;

g)Hydraulic hose pipe (Different sizes) – 2 set;

h) Panel board – 1 set.




As there was no other issues to be discussed /clarified, the meeting ended with votes of thanks form the chair.

                                                                                                                               Signed/-
21/09/2011
(Sunil Baran Debroy)

Addl. Chief Engineer,

&

Project Director,

KKRMP, BWDB, Dhaka.
