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Memo.No.T-6/1563






                        Dated : 02-11-2011

AMENDMENT NO.02 OF TENDER NO.01/2011-2012.


  This is to inform all concern that due to unavoidable circumstances the Tender Notice for invitation of Tender No.01/2011-2012 circulated vide this office Memo.No.T-6/1426 dated 10-10-2011 has amended as follows :

	Sl.

No.
	Item
	Original
	Amendment

	1.
	In Tender documents

Section 6 

Bill of Quantities

Tender No.01/ 2011-12 Package No. W1-COMD-2/2011-12
	In tender documents

 Page No.33 Tender No.01/2010-11 

Package No. W1-COMD-2/2011-12
	In tender document

 Page No.33 Tender No.01/2011-12 

Package  No. W1-COMD-2/2011-12

	2.
	
	In tender document,  Page No.35 

In  Sl./code No.08/40-485-30; Geo-bag size 1030mmx700mm – 3.00m geo fabrics, fill vol.=0.084 cum, wt. = 126.00 Kg
	In tender document,  Page No.35 

In  Sl./code No.08/40-485-30; Geo-bag size 900mmx700mm, geo - fabrics, th.=>3.00, fill vol.=0.0840 cum, wt. = 125.00 Kg

	3.
	
	In tender documents

 Page No.35, In  Sl./code No.09/40-490-30;

Geo-bag size 1030mmx700mm – 3.00m geo fabrics, fill vol.=0.084 cum, wt. = 126.00 Kg
	In tender document,  Page No.35, In  Sl./code No.09/40-490-30; Geo- bag size 900mmx700mm, 

geo fabrics, th.=>3.00, fill vol.=0.0840 cum, wt. = 125.00 Kg

	4.
	
	In tender documents

 Page No.36, In  Sl./code No.10/40-487-30;

Dumping of sand filled geo-bags from properly positioned and anchored flat top barge/pontoon over an area specified by the bathymetric survey for uniform area coverage along the bank line up to the designed length towards river, making  a provisional falling apron at the river end of area coverage, recording the position of dumping barge by a total station etc. complete including loading, unloading sequential piling of geo-bags on the dumping edge of pontoon/ barge, carrying geo-bags from stack yard to dumping place by head load  and power driven flat top country boat etc. complete including higher charge and mobilization of all equipments, materials, labours, taxes, incidental charges but excluding cost of sand filled geo-bags(item 40-490) as per technical specification approved design and direction of Engineer-in-charge.

Geo-bag(1030mmx700mm),geo-fabrics, th. =>3.00mm.Fill vol.=0.084 cum wt. = 126 Kg


	In tender documents

 Page No.36, In  Sl./code No.10/40-495-30

Dumping of sand filled geo-bags along the eroding river bank over  an area specified by design from a flat top barge/pontoon or flat top engines boat including carrying the sand filled geo bags from the stack yard, monitoring and recording the position of dumping boat by total station etc. complete including higher charge and mobilization of all equipments, materials labours, taxes, incidental charges but excluding cost of sand filled geo-bags(item 40-490) as per design, technical specification and detailed drawing included in the tender documents etc. complete as per direction of Engineer-in-charge.

Geo-bag(900mmx700mm),geo-fabrics th.=>3.00mm.  

``Fill vol.=0.084 cum wt. = 125 Kg



	5.
	In Tender documents

Section 6:  

Bill of Quantities

Tender No.01/
2011-12 Package No. W2-COMD-2/ 2011-12
	In tender documents

 Page No.33 Tender No.01/2010-11 Packagae No. W2-COMD-2/2011-12
	In tender documents

Page No.33 Tender No.01/2011-12 Packagae No. W2-COMD-2/ 2011-12

	6.
	
	In tender documents

 Page No.35, In  Sl./code No.09/40-485-30;

Geo-bag size 1030mmx700mm – 3.00m geo fasbrics, fill vol.=0.084 cum, wt. = 126.00 Kg
	In tender documents

 Page No.35, In  Sl./code No.09/40-485-30;

Geo-bag size 900mmx700mm, geo bag fabrics, th.=>3.00, fill vol.=0.0840 cum, wt. = 125.00 Kg

	7.
	
	In tender documents

 Page No.35, In  Sl./code No.10/40-490-30;

Geo-bag size 1030mmx700mm – 3.00m geo fasbrics, fill vol.=0.084 cum, wt. = 126.00 Kg
	In tender documents

 Page No.35, In  Sl./code No.10/40-490-30;

Geo-bag size 900mmx700mm, geo bag fabrics, th.=>3.00, fill vol.=0.0840 cum, wt. = 125.00 Kg

	8.
	
	In tender documents

 Page No.36, In  Sl./code No.11/40-487-30;

Dumping of sand filled geo-bags from properly positioned and anchored flat top barge/pontoon over an area specified by the bathymetric survey for uniform area coverage along the bank line up to the designed length towards river, making  a provisional falling apron at the river end of area coverage, recording the position of dumping barge by a total station etc. complete including loading, unloading sequential piling of geo-bags on the dumping edge of pontoon/ barge, carrying geo-bags from stack yard to dumping place by head load  and power driven flat top country boat etc. complete including higher charge and mobilization of all equipments, materials, labours, taxes, incidental charges but excluding cost of sand filled geo-bags(item 40-490) as per technical specification approved design and direction of Engineer-in-charge.

Geo-bag(1030mmx700mm),geo-fabrics th.=>3.00mm.  

Fill vol.=0.084 cum wt. = 126 Kg


	In tender documents

 Page No.36, In  Sl./code No.11/40-495-30;

Dumping of sand filled geo-bags along the eroding river bank over  an area specified by design from a flat top barge/pontoon or flat top engines boat including carrying the sand filled geo bags from the stack yard, monitoring and recording the position of dumping boat by total station etc. complete including higher charge and mobilization of all equipments, materials labours, taxes, incidental charges but excluding cost of sand filled geo-bags(item 40-490) as per design, technical specification and detailed drawing included in the tender documents etc. complete as per direction of Engineer-in-charge.

Geo-bag(900mmx700mm),geo-fabrics th.=>3.00mm.  

``Fill vol.=0.084 cum wt. = 125 Kg




All other terms and conditions of the tender notice will remain  unchanged and this amendment Notice No.01 will also a part of the tender document of Tender Notice No.01/2011-2012.
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(Swapan Kumar Barua)

Executive Engineer

Chittagong O&M Division-II

BWDB,Chittagong.
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    Dated :.   02 -11-2011
Copy forwarded for favor of information and necessary action to:- 
1. The Chief Engineer, South Eastern Zone, BWDB, Chittagong. 

2. The Superintending Engineer, Chittagong O & M Circle, BWDB, Chittagong. 

3. The Director, Contract & Procurement Cell, BWDB, WAPDA Bhaban, Motijheel, Dhaka. 

4. The Director, Directorate of O&M, BWDB, Dhaka.

5. The Director, Publication Cell, BWDB, WAPDA Bhaban, Motijheel C/A, Dhaka. 

6. The Deputy Commissioner, Chittagong.

7. The Superintendent of Police, Chittagong.

8. The CSO to Director General, BWDB, Dhaka.

9. The Executive Engineer, LGED, Nasirabad, Chittagong.

10. The Deputy Director, DAE, Agrabad, Chittagtong.

11. The Executive Engineer, Chittagong O & M Division - I, BWDB, Chittagong.

12. The Executive Engineer, Cox’s Bazar O & M Division, BWDB, Cox’s Bazar

13. The Executive Engineer, Rangamati  O & M Division , BWDB, Kaptai.

14. The Deputy Director, Regional Accounting Centre, BWDB, Chittagong.

15. The P.S. to Addl. Director General,O&M-1,BWDB,Dhaka.

16. a) The Manager, Sonali Bank Ltd., Bahadderhat Branch, Chittagong.

b) The Deputy General Manager, Janata Bank, Dilkhusha Corporate Branch, 29-Dilkhusha C/A, Dhaka.

17. The Sub Divisional Engineer, Sitakunda / Banskhali / Khagrachari O & M Sub-Division, BWDB, Sitakunda / Banskhali / Khagrachari.

18. The System Analyst, Computer Section, Office of the Chief Monitooring,BWDB, WAPDA Bhavan, Motijheel C/Area, Dhaka. The hard copy and soft copy of the tender notice is enclosed herewith for publication in the BWDB website (Website No.- www.bwdb.gov.bd )
19. The Accountant of RAC, BWDB, Chittagong. He is requested to attend during the opening of tender.

20. Notice Board.

21. M/S...........................................................................

                          (Swapan Kumar Barua)

                                           Executive Engineer

        Chittagong O & M Division-2

            BWDB, Chittagong
