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CORRIGENDUM NO. 01 OF

TENDER NO. 02/2010-2011
This is for all concerned that the Tender Notice No. 02/2010-2011 vide this office memo no. T-2/408 (40)  date : 10-08-2010 has been amended  as follows due to unavoidable circumstances :

	Notice Sl. No.
	Original/Previous
	Amended

	(1)
	(2)
	(3)

	16.
	Last date of tender selling        : 15-09-2010
	Last date of tender selling        : 29-09-2010

	17.
	Last date of tender submission : 16-09-2010
	Last date of tender submission : 30-09-2010

	26.
	Package No. Bhola SII-13 : Supplying non-woven needle punched Geo-bags (empty) Size: 1150 mm ( 800 mm geo-fabrics thickness =3.00 mm fill vol=0.1167 cum weight 175 kg (When filled with dry sand) from km 39.690 to km 41.475 = 1.785 km in connection with “Protection of Shahbazpur Gas Field from Erosion of the Meghna river under Borhanuddin Upazilla of Bhola District (Phase-II)” under Bhola O & M Division-I, BWDB, Bhola during the year 2010-2011.
	Package No. Bhola SII-14 : Supplying non-woven needle punched Geo-bags (empty) Size: 1150 mm ( 800 mm geo-fabrics thickness =3.00 mm fill vol=0.1167 cum weight 175 kg (When filled with dry sand) from km 41.475 to km 42.260 & km 45.285 to km 46.285 = 1.785 km in connection with “Protection of Shahbazpur Gas Field from Erosion of the Meghna river under Borhanuddin Upazilla of Bhola District (Phase-II)” under Bhola O & M Division-I, BWDB, Bhola during the year 2010-2011.

	27.
	Package No. Bhola SII-16 : Supplying non woven needle punched Geo-bage (empty) Size: 1030 mm ( 700 mm geo-febrics thickness =3.00 mm fill vol=0.084 cum weight 126 kg (When filled with dry sand) from km 40.5825 to km 41.475 = 0.8925 km in connection with “Protection of Shahbazpur Gas Field from Erosion of the Meghna river under Borhanuddin Upazilla of Bhola District (Phase-II)” under Bhola O & M Division-I, BWDB, Bhola during the year 2010-2011.
	Package No. Bhola SII-17 : Supplying non woven needle punched Geo-bage (empty) Size: 1030 mm ( 700 mm geo-febrics thickness =3.00 mm fill vol=0.084 cum weight 126 kg (When filled with dry sand) from km 41.475 to km km 42.260 & km 45.285 to km 45.3925 = 0.8925 km in connection with “Protection of Shahbazpur Gas Field from Erosion of the Meghna river under Borhanuddin Upazilla of Bhola District (Phase-II)” under Bhola O & M Division-I, BWDB, Bhola during the year 2010-2011.


“Revised Bill of quantities for Package No. Bhola SII-14 & Bhola SII-17 is available in Banks as mentioned in tender notice no. 02/2010-2011 to be followed instead of original Bill of quantities”.

All others terms & conditions will remain unchanged.

Sd/-


(MD. MAHFUZUR RAHMAN)


Executive Engineer


Bhola O & M Division-I


BWDB, Bhola.






















